S-Index

B E I P R S T V W

## S

sDevice - Static variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
Set_PL2303_BaudRate(PL2303GDriver.BaudRate) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Open an PL2303G USB Device by BaudRate
Set_PL2303_DataBit(PL2303GDriver.DataBits) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Open an PL2303G USB Device by DataBit
Set_PL2303_FlowControl(PL2303GDriver.FlowControl) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Open an PL2303G USB Device by Flow Control mode
Set_PL2303_Parity(PL2303GDriver.Parity) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Open an PL2303G USB Device by Parity
Set_PL2303_StopBit(PL2303GDriver.StopBits) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Open an PL2303G USB Device by StopBit
setDTR(boolean) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Switch PL2303G DTR on or off
setRTS(boolean) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Switch PL2303G RTS on or off
setup(PL2303GDriver.BaudRate, PL2303GDriver.DataBits, PL2303GDriver.StopBits, PL2303GDriver.Parity, PL2303GDriver.FlowControl) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Setup basic communication parameters on PL2303G chip

B E I P R S T V W